


Brushless Motor Images:


Symbol:







1 V, 1 pin







-1 V, 1 pin:










2 V, 1 pin:







-1 V:







Battery voltage level detector:






LCD:







LED picture:




Petentiometer (Low-High):













Switch (Off-On):









Push button (On then Off):

